File: C:\Users\e1286\Documents\MSC_Apex Workspace\Custom Tools 2021.1\Apex Utilities\Fastener Tools\Create Fasteners\Identify Bolts\src\IdentifyBoltsCreate1dConnectors_v02e.py:main 
Output:
Material:       42CrMo4
Fastener type:  Curve Only
Distribution Type:      Compliant - RBE3 
clear_vertex_flag:True
Number of parts : 1480
There are 477 bolt candidates  visible to check 
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_1
####curve name: Curve 23
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_2
####curve name: Curve 24
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_3
####curve name: Curve 25
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_4
####curve name: Curve 26
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_5
####curve name: Curve 27
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_6
####curve name: Curve 28
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999992
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999992
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_7
####curve name: Curve 29
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_8
####curve name: Curve 30
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_9
####curve name: Curve 31
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000041
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000041
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_10
####curve name: Curve 32
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_11
####curve name: Curve 33
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_12
####curve name: Curve 34
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_13
####curve name: Curve 35
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000016
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000016
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_14
####curve name: Curve 36
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_15
####curve name: Curve 37
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_16
####curve name: Curve 38
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000041
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000041
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_17
####curve name: Curve 39
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_18
####curve name: Curve 40
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_19
####curve name: Curve 41
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_20
####curve name: Curve 42
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_21
####curve name: Curve 43
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_22
####curve name: Curve 44
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_23
####curve name: Curve 45
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_24
####curve name: Curve 46
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_25
####curve name: Curve 47
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_26
####curve name: Curve 48
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_27
####curve name: Curve 49
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_29
####curve name: Curve 50
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_30
####curve name: Curve 51
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_31
####curve name: Curve 52
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_32
####curve name: Curve 53
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_33
####curve name: Curve 54
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_34
####curve name: Curve 55
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_35
####curve name: Curve 56
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999967
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999967
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_36
####curve name: Curve 57
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_37
####curve name: Curve 58
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_38
####curve name: Curve 59
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999963
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999963
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_39
####curve name: Curve 60
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_40
####curve name: Curve 61
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_41
####curve name: Curve 62
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_42
####curve name: Curve 63
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_43
####curve name: Curve 64
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_44
####curve name: Curve 65
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_45
####curve name: Curve 66
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_46
####curve name: Curve 67
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_47
####curve name: Curve 68
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_48
####curve name: Curve 69
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_49
####curve name: Curve 70
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_50
####curve name: Curve 71
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_51
####curve name: Curve 72
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_52
####curve name: Curve 73
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_53
####curve name: Curve 74
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_54
####curve name: Curve 75
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_55
####curve name: Curve 76
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_56
####curve name: Curve 77
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_57
####curve name: Curve 78
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_58
####curve name: Curve 79
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000034
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000034
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_59
####curve name: Curve 80
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_60
####curve name: Curve 81
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_61
####curve name: Curve 82
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_62
####curve name: Curve 83
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_63
####curve name: Curve 84
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_64
####curve name: Curve 85
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_65
####curve name: Curve 86
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_66
####curve name: Curve 87
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_67
####curve name: Curve 88
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_68
####curve name: Curve 89
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_69
####curve name: Curve 90
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_70
####curve name: Curve 91
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_71
####curve name: Curve 92
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_72
####curve name: Curve 93
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_73
####curve name: Curve 94
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_74
####curve name: Curve 95
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_75
####curve name: Curve 96
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_76
####curve name: Curve 97
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_77
####curve name: Curve 98
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_78
####curve name: Curve 99
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_79
####curve name: Curve 100
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_80
####curve name: Curve 101
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_81
####curve name: Curve 102
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_82
####curve name: Curve 103
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_83
####curve name: Curve 104
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_84
####curve name: Curve 105
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_85
####curve name: Curve 106
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_86
####curve name: Curve 107
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_87
####curve name: Curve 108
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_88
####curve name: Curve 109
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_89
####curve name: Curve 110
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_90
####curve name: Curve 111
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_91
####curve name: Curve 112
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000024
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_92
####curve name: Curve 113
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_93
####curve name: Curve 114
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_94
####curve name: Curve 115
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_95
####curve name: Curve 116
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_96
####curve name: Curve 117
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_97
####curve name: Curve 118
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_98
####curve name: Curve 119
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_99
####curve name: Curve 120
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_100
####curve name: Curve 121
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_101
####curve name: Curve 122
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_102
####curve name: Curve 123
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_103
####curve name: Curve 124
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_104
####curve name: Curve 125
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_105
####curve name: Curve 126
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_106
####curve name: Curve 127
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_107
####curve name: Curve 128
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_108
####curve name: Curve 129
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_109
####curve name: Curve 130
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_110
####curve name: Curve 131
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_111
####curve name: Curve 132
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_112
####curve name: Curve 133
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_113
####curve name: Curve 134
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_114
####curve name: Curve 135
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_115
####curve name: Curve 136
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_116
####curve name: Curve 137
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_117
####curve name: Curve 138
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_118
####curve name: Curve 139
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_119
####curve name: Curve 140
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_120
####curve name: Curve 141
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_121
####curve name: Curve 142
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_122
####curve name: Curve 143
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_123
####curve name: Curve 144
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_124
####curve name: Curve 145
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_125
####curve name: Curve 146
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_126
####curve name: Curve 147
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_127
####curve name: Curve 148
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_128
####curve name: Curve 149
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_129
####curve name: Curve 150
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_130
####curve name: Curve 151
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_131
####curve name: Curve 152
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_132
####curve name: Curve 153
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_133
####curve name: Curve 154
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_134
####curve name: Curve 155
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_135
####curve name: Curve 156
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_136
####curve name: Curve 157
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_137
####curve name: Curve 158
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_138
####curve name: Curve 159
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_139
####curve name: Curve 160
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999977
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_140
####curve name: Curve 161
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000027
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000027
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_141
####curve name: Curve 162
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_142
####curve name: Curve 163
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999974
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_143
####curve name: Curve 164
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000016
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000016
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_144
####curve name: Curve 165
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_145
####curve name: Curve 166
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_146
####curve name: Curve 167
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_147
####curve name: Curve 168
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999995
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_148
####curve name: Curve 169
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999981
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999981
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_149
####curve name: Curve 170
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_150
####curve name: Curve 171
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_151
####curve name: Curve 172
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000001
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_152
####curve name: Curve 173
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999988
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_153
####curve name: Curve 174
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_154
####curve name: Curve 175
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_155
####curve name: Curve 176
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.31000000000003
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_156
####curve name: Curve 177
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000002
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_157
####curve name: Curve 178
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000013
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_158
####curve name: Curve 179
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999999
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_159
####curve name: Curve 180
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000016
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.310000000000016
Washer Failed Check 1a
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 2
I am in checking verts
Number of Cylindrical Faces: 3
Diameter 32.00002702926651 bolt stem index=11
Tolerance: 6.0
Number of Concentric Faces: 9
Number of Edges 10
BoltType: Type122
solid: STUD-M39X700
=====================================
Type 132 Romacs Stud
Head heigt               0.00    
Bolt length              700.00  
Bolt diam                39.00   
part name: Pitch/Blade Studs/STUD-M39X700.PRT_160
####curve name: Curve 181
Len of proxy solids: 2
No of near solids:2
===== Identifying nuts======
Nut Failed Check 1a 5  faces
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999981
I am in checking verts
Washer Pass Check 1a
Washer Pass Check 1b- chamfered washer
Identified Washer
Washer height:     6.60
Washer outer dia:    72.01
Washer inner dia:    40.00
===== Identifying nuts======
I am in checking verts
Nut passed Check 1a
There are 22edges for nut candidate
pass Check 1c    c
No of Faces: 11
No of CircularFaces: 0
Number of Cylindrical Faces: 1
No of CircularFaces: 0
No of ConcentricFaces: 5
=====Identified nut=======
Nut Type: hex Nut height:    33.40
Nut outer dia:    55.91
Nut inner dia:    34.10
===== Identifying washers
bolt_length:   700.00
Using tolerance: 15.309999999999981
Washer Failed Check 1a
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 5 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
 I am in 1
Number of Faces 11 faces
Number of Circular Faces: 0
============SUMMARY==================
Number of solids in model        : 2463
Number of visible solids searched: 477

Bolt Type  Number 
-------------------
      m39:      159

