NASTRAN
SOL 103
$ Direct Text Input for Executive Control
CEND
TITLE = MSC.Nastran job to generate mnf exported from Apex Utils
ECHO = NONE
$ Direct Text Input for Global Case Control Data
ADAMSMNF FLEXBODY=YES,FLEXONLY=YES,OUTGSTRS=YES,
$

$ Comment if stresses are not required
$OUTSTRS=YES
SET 1 = 1,2
GPSTRESS(PLOT) = 1
STRESS(PLOT,SORT1,REAL,VONMISES,BILIN)=ALL
STRFIELD = ALL
$STRESS(PLOT) = ALL
$STRAIN(PLOT) = ALL
$GPSTRESS(PLOT) = ALL
$GPSTRAIN(PLOT) = ALL
$
SUBTITLE=Default
METHOD = 1

$ Define surface for stress and strain grid shapes
$
OUTPUT(POST)
SET 2 = ALL
VOLUME 1 SET 2,PRINCIPAL,SYSTEM CORD 0
SET 3 = ALL
SURFACE 2 SET 3,FIBRE ALL,SYSTEM CORD 0,AXIS X1,NORMAL R,
TOPOLOGICAL,BRANCH BREAK


BEGIN BULK
$PARAM,AUTOMSET,LUSOL $ Use for nastran v2017
$PARAM,AUTOMSET,YES    $ Use for nastran previous to 2017
$PARAM,POST,0
DTI,UNITS,1,MGG,N,MM,S
